Cable Length Effect on Stepper Motor Power Supply and IIC Lines

**Power Supply Voltage When Supplied Directly (Picture 1)**

Graphical user interface

Description automatically generated

Voltage supplied is 12V.

**Power Supply Voltage When Ran Through 340cm of Cable and IIC Clock (Picture 2)**

A picture containing text

Description automatically generated

IIC clock speed is 100kHz.